/**
 * Marlin 3D Printer Firmware
 * Copyright (c) 2020 MarlinFirmware [https://github.com/MarlinFirmware/Marlin]
 *
 * Based on Sprinter and grbl.
 * Copyright (c) 2011 Camiel Gubbels / Erik van der Zalm
 *
 * This program is free software: you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation, either version 3 of the License, or
 * (at your option) any later version.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 *
 * You should have received a copy of the GNU General Public License
 * along with this program.  If not, see <https://www.gnu.org/licenses/>.
 *
 */
#pragma once

/**
 * Arduino Mega with RAMPS v1.4 (or v1.3) pin assignments
 *
 * Applies to the following boards:
 *
 *  RAMPS_14_EFB (Hotend, Fan, Bed)
 *  RAMPS_14_EEB (Hotend0, Hotend1, Bed)
 *  RAMPS_14_EFF (Hotend, Fan0, Fan1)
 *  RAMPS_14_EEF (Hotend0, Hotend1, Fan)
 *  RAMPS_14_SF  (Spindle, Controller Fan)
 *
 *  RAMPS_13_EFB (Hotend, Fan, Bed)
 *  RAMPS_13_EEB (Hotend0, Hotend1, Bed)
 *  RAMPS_13_EFF (Hotend, Fan0, Fan1)
 *  RAMPS_13_EEF (Hotend0, Hotend1, Fan)
 *  RAMPS_13_SF  (Spindle, Controller Fan)
 *
 *  Other pins_MYBOARD.h files may override these defaults
 *
 *  Differences between
 *  RAMPS_13 | RAMPS_14
 *         7 | 11
 */

#if ENABLED(AZSMZ_12864) && DISABLED(ALLOW_SAM3X8E)
  #error "No pins defined for RAMPS with AZSMZ_12864."
#endif

#include "env_validate.h"

// Custom flags and defines for the build
//#define BOARD_CUSTOM_BUILD_FLAGS -D__FOO__

#ifndef BOARD_INFO_NAME
  #define BOARD_INFO_NAME "RAMPS 1.4"
#endif

//
// Servos
//
#ifndef SERVO0_PIN
  #ifdef IS_RAMPS_13
    #define SERVO0_PIN                         7
  #else
    #define SERVO0_PIN                        11
  #endif
#endif
#ifndef SERVO1_PIN
  #define SERVO1_PIN                           6
#endif
#ifndef SERVO2_PIN
  #define SERVO2_PIN                           5
#endif
#ifndef SERVO3_PIN
  #define SERVO3_PIN                           4
#endif

//
// Limit Switches
//
#ifndef X_STOP_PIN
  #ifndef X_MIN_PIN
    #define X_MIN_PIN                          3
  #endif
  #ifndef X_MAX_PIN
    #define X_MAX_PIN                          2
  #endif
#endif
#ifndef Y_STOP_PIN
  #ifndef Y_MIN_PIN
    #define Y_MIN_PIN                         14
  #endif
  #ifndef Y_MAX_PIN
    #define Y_MAX_PIN                         15
  #endif
#endif
#ifndef Z_STOP_PIN
  #ifndef Z_MIN_PIN
    #define Z_MIN_PIN                         18
  #endif
  #ifndef Z_MAX_PIN
    #define Z_MAX_PIN                         19
  #endif
#endif

//
// Z Probe (when not Z_MIN_PIN)
//
#ifndef Z_MIN_PROBE_PIN
  #define Z_MIN_PROBE_PIN                     32
#endif

//
// Steppers
//
#define X_STEP_PIN                            54
#define X_DIR_PIN                             55
#define X_ENABLE_PIN                          38
#ifndef X_CS_PIN
  #define X_CS_PIN                   AUX3_03_PIN
#endif

#define Y_STEP_PIN                            60
#define Y_DIR_PIN                             61
#define Y_ENABLE_PIN                          56
#ifndef Y_CS_PIN
  #define Y_CS_PIN                   AUX3_07_PIN
#endif

#ifndef Z_STEP_PIN
  #define Z_STEP_PIN                          46
#endif
#ifndef Z_DIR_PIN
  #define Z_DIR_PIN                           48
#endif
#ifndef Z_ENABLE_PIN
  #define Z_ENABLE_PIN                        62
#endif
#ifndef Z_CS_PIN
  #define Z_CS_PIN                            40
#endif

#ifndef E0_STEP_PIN
  #define E0_STEP_PIN                         26
#endif
#ifndef E0_DIR_PIN
  #define E0_DIR_PIN                          28
#endif
#ifndef E0_ENABLE_PIN
  #define E0_ENABLE_PIN                       24
#endif
#ifndef E0_CS_PIN
  #define E0_CS_PIN                           42
#endif

#ifndef E1_STEP_PIN
  #define E1_STEP_PIN                         36
#endif
#ifndef E1_DIR_PIN
  #define E1_DIR_PIN                          34
#endif
#ifndef E1_ENABLE_PIN
  #define E1_ENABLE_PIN                       30
#endif
#ifndef E1_CS_PIN
  #define E1_CS_PIN                           44
#endif

//
// Temperature Sensors
//
#ifndef TEMP_0_PIN
  #define TEMP_0_PIN                          13  // Analog Input
#endif
#ifndef TEMP_1_PIN
  #define TEMP_1_PIN                          15  // Analog Input
#endif
#ifndef TEMP_BED_PIN
  #define TEMP_BED_PIN                        14  // Analog Input
#endif

//
// SPI for MAX Thermocouple
//
#ifndef TEMP_0_CS_PIN
  #define TEMP_0_CS_PIN                       66  // Don't use 53 if using Display/SD card (SDSS) or 49 (SD_DETECT_PIN)
#endif

//
// Heaters / Fans
//
#ifndef MOSFET_A_PIN
  #define MOSFET_A_PIN                        10
#endif
#ifndef MOSFET_B_PIN
  #define MOSFET_B_PIN                         9
#endif
#ifndef MOSFET_C_PIN
  #define MOSFET_C_PIN                         8
#endif
#ifndef MOSFET_D_PIN
  #define MOSFET_D_PIN                        -1
#endif

#define HEATER_0_PIN                MOSFET_A_PIN

#if FET_ORDER_EFB                                 // Hotend, Fan, Bed
  #define HEATER_BED_PIN            MOSFET_C_PIN
#elif FET_ORDER_EEF                               // Hotend, Hotend, Fan
  #define HEATER_1_PIN              MOSFET_B_PIN
#elif FET_ORDER_EEB                               // Hotend, Hotend, Bed
  #define HEATER_1_PIN              MOSFET_B_PIN
  #define HEATER_BED_PIN            MOSFET_C_PIN
#elif FET_ORDER_EFF                               // Hotend, Fan, Fan
  #define FAN1_PIN                  MOSFET_C_PIN
#elif DISABLED(FET_ORDER_SF)                      // Not Spindle, Fan (i.e., "EFBF" or "EFBE")
  #define HEATER_BED_PIN            MOSFET_C_PIN
  #if EITHER(HAS_MULTI_HOTEND, HEATERS_PARALLEL)
    #define HEATER_1_PIN            MOSFET_D_PIN
  #else
    #define FAN1_PIN                MOSFET_D_PIN
  #endif
#endif

#ifndef FAN_PIN
  #if EITHER(FET_ORDER_EFB, FET_ORDER_EFF)        // Hotend, Fan, Bed or Hotend, Fan, Fan
    #define FAN_PIN                 MOSFET_B_PIN
  #elif EITHER(FET_ORDER_EEF, FET_ORDER_SF)       // Hotend, Hotend, Fan or Spindle, Fan
    #define FAN_PIN                 MOSFET_C_PIN
  #elif FET_ORDER_EEB                             // Hotend, Hotend, Bed
    #define FAN_PIN                            4  // IO pin. Buffer needed
  #else                                           // Non-specific are "EFB" (i.e., "EFBF" or "EFBE")
    #define FAN_PIN                 MOSFET_B_PIN
  #endif
#endif

//
// Misc. Functions
//
#ifndef SDSS
  #define SDSS                       AUX3_03_PIN
#endif
#define LED_PIN                               13

#ifndef FILWIDTH_PIN
  #define FILWIDTH_PIN                         5  // Analog Input on AUX2
#endif

// RAMPS 1.4 DIO 4 on the servos connector
#ifndef FIL_RUNOUT_PIN
  #define FIL_RUNOUT_PIN                       4
#endif

#ifndef PS_ON_PIN
  #define PS_ON_PIN                           12
#endif

#if ENABLED(CASE_LIGHT_ENABLE) && !defined(CASE_LIGHT_PIN) && !defined(SPINDLE_LASER_ENA_PIN)
  #if NUM_SERVOS <= 1                             // Prefer the servo connector
    #define CASE_LIGHT_PIN                     6  // Hardware PWM
  #elif HAS_FREE_AUX2_PINS
    #define CASE_LIGHT_PIN                    44  // Hardware PWM
  #endif
#endif

//
// M3/M4/M5 - Spindle/Laser Control
//
#if HAS_CUTTER && !defined(SPINDLE_LASER_ENA_PIN)
  #if !NUM_SERVOS                                 // Use servo connector if possible
    #define SPINDLE_LASER_ENA_PIN              4  // Pullup or pulldown!
    #define SPINDLE_LASER_PWM_PIN              6  // Hardware PWM
    #define SPINDLE_DIR_PIN                    5
  #elif HAS_FREE_AUX2_PINS
    #define SPINDLE_LASER_ENA_PIN             40  // Pullup or pulldown!
    #define SPINDLE_LASER_PWM_PIN             44  // Hardware PWM
    #define SPINDLE_DIR_PIN                   65
  #else
    #error "No auto-assignable Spindle/Laser pins available."
  #endif
#endif

//
// TMC software SPI
//
#if ENABLED(TMC_USE_SW_SPI)
  #ifndef TMC_SW_MOSI
    #define TMC_SW_MOSI                       66
  #endif
  #ifndef TMC_SW_MISO
    #define TMC_SW_MISO                       44
  #endif
  #ifndef TMC_SW_SCK
    #define TMC_SW_SCK                        64
  #endif
#endif

#if HAS_TMC_UART
  /**
   * TMC2208/TMC2209 stepper drivers
   *
   * Hardware serial communication ports.
   * If undefined software serial is used according to the pins below
   *
   * Serial2 -- AUX-4 Pin 18 (D16 TX2) and AUX-4 Pin 17 (D17 RX2)
   * Serial1 -- Pins D18 and D19 are used for Z-MIN and Z-MAX
   */
  //#define X_HARDWARE_SERIAL Serial1
  //#define X2_HARDWARE_SERIAL Serial1
  //#define Y_HARDWARE_SERIAL Serial1
  //#define Y2_HARDWARE_SERIAL Serial1
  //#define Z_HARDWARE_SERIAL Serial1
  //#define Z2_HARDWARE_SERIAL Serial1
  //#define E0_HARDWARE_SERIAL Serial1
  //#define E1_HARDWARE_SERIAL Serial1
  //#define E2_HARDWARE_SERIAL Serial1
  //#define E3_HARDWARE_SERIAL Serial1
  //#define E4_HARDWARE_SERIAL Serial1

  #ifndef X_SERIAL_TX_PIN
    #define X_SERIAL_TX_PIN                   40
  #endif
  #ifndef X_SERIAL_RX_PIN
    #define X_SERIAL_RX_PIN                   63
  #endif
  #ifndef X2_SERIAL_TX_PIN
    #define X2_SERIAL_TX_PIN                  -1
  #endif
  #ifndef X2_SERIAL_RX_PIN
    #define X2_SERIAL_RX_PIN                  -1
  #endif

  #ifndef Y_SERIAL_TX_PIN
    #define Y_SERIAL_TX_PIN                   59
  #endif
  #ifndef Y_SERIAL_RX_PIN
    #define Y_SERIAL_RX_PIN                   64
  #endif
  #ifndef Y2_SERIAL_TX_PIN
    #define Y2_SERIAL_TX_PIN                  -1
  #endif
  #ifndef Y2_SERIAL_RX_PIN
    #define Y2_SERIAL_RX_PIN                  -1
  #endif

  #ifndef Z_SERIAL_TX_PIN
    #define Z_SERIAL_TX_PIN                   42
  #endif
  #ifndef Z_SERIAL_RX_PIN
    #define Z_SERIAL_RX_PIN                   65
  #endif
  #ifndef Z2_SERIAL_TX_PIN
    #define Z2_SERIAL_TX_PIN                  -1
  #endif
  #ifndef Z2_SERIAL_RX_PIN
    #define Z2_SERIAL_RX_PIN                  -1
  #endif

  #ifndef E0_SERIAL_TX_PIN
    #define E0_SERIAL_TX_PIN                  44
  #endif
  #ifndef E0_SERIAL_RX_PIN
    #define E0_SERIAL_RX_PIN                  66
  #endif
  #ifndef E1_SERIAL_TX_PIN
    #define E1_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E1_SERIAL_RX_PIN
    #define E1_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E2_SERIAL_TX_PIN
    #define E2_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E2_SERIAL_RX_PIN
    #define E2_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E3_SERIAL_TX_PIN
    #define E3_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E3_SERIAL_RX_PIN
    #define E3_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E4_SERIAL_TX_PIN
    #define E4_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E4_SERIAL_RX_PIN
    #define E4_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E5_SERIAL_TX_PIN
    #define E5_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E5_SERIAL_RX_PIN
    #define E5_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E6_SERIAL_TX_PIN
    #define E6_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E6_SERIAL_RX_PIN
    #define E6_SERIAL_RX_PIN                  -1
  #endif
  #ifndef E7_SERIAL_TX_PIN
    #define E7_SERIAL_TX_PIN                  -1
  #endif
  #ifndef E7_SERIAL_RX_PIN
    #define E7_SERIAL_RX_PIN                  -1
  #endif
#endif

//
// Průša i3 MK2 Multiplexer Support
//
#ifndef E_MUX0_PIN
  #define E_MUX0_PIN                          40  // Z_CS_PIN
#endif
#ifndef E_MUX1_PIN
  #define E_MUX1_PIN                          42  // E0_CS_PIN
#endif
#ifndef E_MUX2_PIN
  #define E_MUX2_PIN                          44  // E1_CS_PIN
#endif

//
// AUX3 : GND D52 D50 5V
//        NC  D53 D51 D49

#define AUX3_03_PIN                           53
#define AUX3_04_PIN                           52
#define AUX3_05_PIN                           51
#define AUX3_06_PIN                           50
#define AUX3_07_PIN                           49

//
// AUX4 : D16 D17 D23 D25 D27 D29 D31 D33 D35 D37 D39 D41 D43 D45 D47 D32 GND 5V
//

#define AUX4_03_PIN                           32
#define AUX4_04_PIN                           47
#define AUX4_05_PIN                           45
#define AUX4_06_PIN                           43
#define AUX4_07_PIN                           41
#define AUX4_08_PIN                           39
#define AUX4_09_PIN                           37
#define AUX4_10_PIN                           35
#define AUX4_11_PIN                           33
#define AUX4_12_PIN                           31
#define AUX4_13_PIN                           29
#define AUX4_14_PIN                           27
#define AUX4_15_PIN                           25
#define AUX4_16_PIN                           23
#define AUX4_17_PIN                           17
#define AUX4_18_PIN                           16

/**
 * LCD adapter. NOTE: These come in two variants. The socket keys can be
 * on either side, and may be backwards on some boards / displays.
 *         ------                     ------
 *    D37 |10  9 | D35    (MISO) D50 |10  9 | D52 (SCK)
 *    D17 | 8  7 | D16           D31 | 8  7 | D53
 *    D23   6  5   D25           D33   6  5   D51 (MOSI)
 *    D27 | 4  3 | D29           D49 | 4  3 | D41
 *    GND | 2  1 | 5V            GND | 2  1 | NC
 *         ------                     ------
 *          EXP1                       EXP2
 */
#ifndef EXP1_03_PIN
  #define EXP1_03_PIN                AUX4_13_PIN
  #define EXP1_04_PIN                AUX4_14_PIN
  #define EXP1_05_PIN                AUX4_15_PIN
  #define EXP1_06_PIN                AUX4_16_PIN
  #define EXP1_07_PIN                AUX4_18_PIN
  #define EXP1_08_PIN                AUX4_17_PIN
  #define EXP1_09_PIN                AUX4_10_PIN
  #define EXP1_10_PIN                AUX4_09_PIN

  #define EXP2_03_PIN                AUX4_07_PIN
  #define EXP2_04_PIN                AUX3_07_PIN
  #define EXP2_05_PIN                AUX3_05_PIN
  #define EXP2_06_PIN                AUX4_11_PIN
  #define EXP2_07_PIN                AUX3_03_PIN
  #define EXP2_08_PIN                AUX4_12_PIN
  #define EXP2_09_PIN                AUX3_04_PIN
  #define EXP2_10_PIN                AUX3_06_PIN
#endif

//////////////////////////
// LCDs and Controllers //
//////////////////////////

#if HAS_WIRED_LCD

  // Uncomment screen orientation
  //#define LCD_SCREEN_ROT_90
  //#define LCD_SCREEN_ROT_180
  //#define LCD_SCREEN_ROT_270

  //
  // LCD Display output pins
  //
  #if ENABLED(REPRAPWORLD_GRAPHICAL_LCD)

    #define LCD_PINS_RS              EXP2_04_PIN  // CS chip select /SS chip slave select
    #define LCD_PINS_ENABLE          EXP2_05_PIN  // SID (MOSI)
    #define LCD_PINS_D4              EXP2_09_PIN  // SCK (CLK) clock

  #elif BOTH(IS_NEWPANEL, PANEL_ONE)

    #define LCD_PINS_RS                       40
    #define LCD_PINS_ENABLE                   42
    #define LCD_PINS_D4                       65
    #define LCD_PINS_D5                       66
    #define LCD_PINS_D6                       44
    #define LCD_PINS_D7                       64

  #elif ENABLED(TFTGLCD_PANEL_SPI)

    #define TFTGLCD_CS               EXP2_06_PIN

  #else

    #if ENABLED(CR10_STOCKDISPLAY)

      #define LCD_PINS_RS            EXP1_04_PIN
      #define LCD_PINS_ENABLE        EXP1_03_PIN
      #define LCD_PINS_D4            EXP1_05_PIN

      #if !IS_NEWPANEL
        #define BEEPER_PIN           EXP1_10_PIN
      #endif

    #elif ENABLED(ZONESTAR_LCD)

      #error "CAUTION! ZONESTAR_LCD on RAMPS requires wiring modifications. It plugs into AUX2 but GND and 5V need to be swapped. Comment out this line to continue."
      #define LCD_PINS_RS                     64
      #define LCD_PINS_ENABLE                 44
      #define LCD_PINS_D4                     63
      #define LCD_PINS_D5                     40
      #define LCD_PINS_D6                     42
      #define LCD_PINS_D7                     65

    #else

      #if EITHER(MKS_12864OLED, MKS_12864OLED_SSD1306)
        #define LCD_PINS_DC          EXP1_05_PIN  // Set as output on init
        #define LCD_PINS_RS          EXP1_04_PIN  // Pull low for 1s to init
        // DOGM SPI LCD Support
        #define DOGLCD_A0            LCD_PINS_DC
        #define DOGLCD_CS            EXP1_07_PIN
        #define DOGLCD_MOSI          EXP1_08_PIN
        #define DOGLCD_SCK           EXP1_06_PIN
      #else
        #define LCD_PINS_RS          EXP1_07_PIN
        #define LCD_PINS_ENABLE      EXP1_08_PIN
        #define LCD_PINS_D4          EXP1_06_PIN
        #define LCD_PINS_D5          EXP1_05_PIN
        #define LCD_PINS_D6          EXP1_04_PIN
      #endif

      #define LCD_PINS_D7            EXP1_03_PIN

      #if !IS_NEWPANEL
        #define BEEPER_PIN           EXP2_06_PIN
      #endif

    #endif

    #if !IS_NEWPANEL
      // Buttons attached to a shift register
      // Not wired yet
      //#define SHIFT_CLK_PIN                 38
      //#define SHIFT_LD_PIN                  42
      //#define SHIFT_OUT_PIN                 40
      //#define SHIFT_EN_PIN         EXP1_08_PIN
    #endif

  #endif

  #if ENABLED(REPRAP_DISCOUNT_FULL_GRAPHIC_SMART_CONTROLLER)
    #define BTN_ENC_EN               LCD_PINS_D7  // Detect the presence of the encoder
  #endif

  //
  // LCD Display input pins
  //
  #if IS_NEWPANEL

    #if IS_RRD_SC

      #define BEEPER_PIN             EXP1_10_PIN

      #if ENABLED(CR10_STOCKDISPLAY)
        #define BTN_EN1              EXP1_08_PIN
        #define BTN_EN2              EXP1_06_PIN
      #else
        #define BTN_EN1              EXP2_08_PIN
        #define BTN_EN2              EXP2_06_PIN
      #endif

      #define BTN_ENC                EXP1_09_PIN
      #ifndef SD_DETECT_PIN
        #define SD_DETECT_PIN        EXP2_04_PIN
      #endif
      #ifndef KILL_PIN
        #define KILL_PIN             EXP2_03_PIN
      #endif

      #if ENABLED(BQ_LCD_SMART_CONTROLLER)
        #define LCD_BACKLIGHT_PIN    AUX4_08_PIN
      #endif

    #elif ENABLED(REPRAPWORLD_GRAPHICAL_LCD)

      #define BTN_EN1                         64
      #define BTN_EN2                         59
      #define BTN_ENC                         63
      #define SD_DETECT_PIN                   42

    #elif ENABLED(LCD_I2C_PANELOLU2)

      #define BTN_EN1                AUX4_04_PIN
      #define BTN_EN2                AUX4_06_PIN
      #define BTN_ENC                AUX4_03_PIN
      #define LCD_SDSS                      SDSS
      #define KILL_PIN               EXP2_03_PIN

    #elif ENABLED(LCD_I2C_VIKI)

      #define BTN_EN1                         40  // https://files.panucatt.com/datasheets/viki_wiring_diagram.pdf explains 40/42.
      #define BTN_EN2                         42
      #define BTN_ENC                         -1

      #define LCD_SDSS                      SDSS
      #define SD_DETECT_PIN          EXP2_04_PIN

    #elif ANY(VIKI2, miniVIKI)

      #define DOGLCD_CS                       45
      #define DOGLCD_A0                       44
      #define LCD_SCREEN_ROT_180

      #define BEEPER_PIN             EXP2_06_PIN
      #define STAT_LED_RED_PIN                32
      #define STAT_LED_BLUE_PIN      EXP1_09_PIN

      #define BTN_EN1                         22
      #define BTN_EN2                          7
      #define BTN_ENC                         39

      #define SD_DETECT_PIN                   -1  // Pin 49 for display SD interface, 72 for easy adapter board
      #define KILL_PIN               EXP2_08_PIN

    #elif ENABLED(ELB_FULL_GRAPHIC_CONTROLLER)

      #define DOGLCD_CS              EXP1_03_PIN
      #define DOGLCD_A0              EXP1_04_PIN

      #define BEEPER_PIN             EXP1_06_PIN
      #define LCD_BACKLIGHT_PIN      EXP2_06_PIN

      #define BTN_EN1                EXP1_09_PIN
      #define BTN_EN2                EXP1_10_PIN
      #define BTN_ENC                EXP2_08_PIN

      #define LCD_SDSS                      SDSS
      #define SD_DETECT_PIN          EXP2_04_PIN
      #define KILL_PIN               EXP2_03_PIN

    #elif EITHER(MKS_MINI_12864, FYSETC_MINI_12864)

      #define BEEPER_PIN             EXP1_10_PIN
      #define BTN_ENC                EXP1_09_PIN
      #ifndef SD_DETECT_PIN
        #define SD_DETECT_PIN        EXP2_04_PIN
      #endif

      #ifndef KILL_PIN
        #define KILL_PIN             EXP2_03_PIN
      #endif

      #if ENABLED(MKS_MINI_12864)

        #define DOGLCD_A0            EXP1_04_PIN
        #define DOGLCD_CS            EXP1_05_PIN

        // not connected to a pin
        #define LCD_BACKLIGHT_PIN             -1  // 65 (MKS mini12864 can't adjust backlight by software!)

        #define BTN_EN1              EXP2_08_PIN
        #define BTN_EN2              EXP2_06_PIN

      #elif ENABLED(FYSETC_MINI_12864)

        // From https://wiki.fysetc.com/Mini12864_Panel/?fbclid=IwAR1FyjuNdVOOy9_xzky3qqo_WeM5h-4gpRnnWhQr_O1Ef3h0AFnFXmCehK8

        #define DOGLCD_A0            EXP1_07_PIN
        #define DOGLCD_CS            EXP1_08_PIN

        #define BTN_EN1              EXP2_06_PIN
        #define BTN_EN2              EXP2_08_PIN

        //#define FORCE_SOFT_SPI                  // Use this if default of hardware SPI causes display problems
                                                  //   results in LCD soft SPI mode 3, SD soft SPI mode 0

        #define LCD_RESET_PIN        EXP1_06_PIN  // Must be high or open for LCD to operate normally.

        #if EITHER(FYSETC_MINI_12864_1_2, FYSETC_MINI_12864_2_0)
          #ifndef RGB_LED_R_PIN
            #define RGB_LED_R_PIN    EXP1_05_PIN
          #endif
          #ifndef RGB_LED_G_PIN
            #define RGB_LED_G_PIN    EXP1_04_PIN
          #endif
          #ifndef RGB_LED_B_PIN
            #define RGB_LED_B_PIN    EXP1_03_PIN
          #endif
        #elif ENABLED(FYSETC_MINI_12864_2_1)
          #define NEOPIXEL_PIN       EXP1_05_PIN
        #endif

      #endif

    #elif ENABLED(MINIPANEL)

      #define BEEPER_PIN                      42
      // not connected to a pin
      #define LCD_BACKLIGHT_PIN               65  // backlight LED on A11/D65

      #define DOGLCD_A0                       44
      #define DOGLCD_CS                       66

      #define BTN_EN1                         40
      #define BTN_EN2                         63
      #define BTN_ENC                         59

      #define SD_DETECT_PIN          EXP2_04_PIN
      #define KILL_PIN                        64

    #elif ENABLED(ZONESTAR_LCD)

      #define ADC_KEYPAD_PIN                  12

    #elif ENABLED(AZSMZ_12864)

      // Pins only defined for RAMPS_SMART currently

    #elif ENABLED(G3D_PANEL)

      #define BEEPER_PIN             EXP2_06_PIN

      #define SD_DETECT_PIN          EXP2_04_PIN
      #define KILL_PIN               EXP2_03_PIN

      #define BTN_EN1                EXP1_10_PIN
      #define BTN_EN2                EXP1_09_PIN
      #define BTN_ENC                EXP2_08_PIN

    #elif IS_TFTGLCD_PANEL

      #define SD_DETECT_PIN          EXP2_04_PIN

    #else

      #define BEEPER_PIN             EXP2_06_PIN

      // Buttons are directly attached to AUX-2
      #if ENABLED(PANEL_ONE)
        #define BTN_EN1                       59  // AUX2 PIN 3
        #define BTN_EN2                       63  // AUX2 PIN 4
        #define BTN_ENC              EXP2_04_PIN
      #else
        #define BTN_EN1              EXP1_10_PIN
        #define BTN_EN2              EXP1_09_PIN
        #define BTN_ENC              EXP2_08_PIN
      #endif

    #endif
  #endif // IS_NEWPANEL

#endif // HAS_WIRED_LCD

#if IS_RRW_KEYPAD && !HAS_ADC_BUTTONS
  #define SHIFT_OUT_PIN                       40
  #define SHIFT_CLK_PIN                       44
  #define SHIFT_LD_PIN                        42
  #ifndef BTN_EN1
    #define BTN_EN1                           64
  #endif
  #ifndef BTN_EN2
    #define BTN_EN2                           59
  #endif
  #ifndef BTN_ENC
    #define BTN_ENC                           63
  #endif
#endif

#if BOTH(TOUCH_UI_FTDI_EVE, LCD_FYSETC_TFT81050)

  #error "CAUTION! LCD_FYSETC_TFT81050 requires wiring modifications. See 'pins_RAMPS.h' for details. Comment out this line to continue."

  /**
   * FYSETC TFT-81050 display pinout
   *
   *               Board                                     Display
   *               -----                                     -----
   *  (SCK)   D52 | 1 2 | D50    (MISO)                MISO | 1 2 | SCK
   *  (SD_CS) D53 | 3 4 | D33 (BNT_EN2) (BNT_EN2) MOD_RESET | 3 4 | SD_CS
   *  (MOSI)  D51 | 5 6   D31 (BNT_EN1) (BNT_EN1)    LCD_CS | 5 6   MOSI
   *        RESET | 7 8 | D49  (SD_DET)              SD_DET | 7 8 | RESET
   *           NC | 9 10| GND                           GND | 9 10| 5V
   *               -----                                     -----
   *                EXP2                                      EXP1
   *
   * Needs custom cable:
   *
   *    Board   Adapter   Display
   *           _________
   *   EXP2-1 ----------- EXP1-10
   *   EXP2-2 ----------- EXP1-9
   *   EXP2-4 ----------- EXP1-8
   *   EXP2-4 ----------- EXP1-7
   *   EXP2-3 ----------- EXP1-6
   *   EXP2-6 ----------- EXP1-5
   *   EXP2-7 ----------- EXP1-4
   *   EXP2-8 ----------- EXP1-3
   *   EXP2-1 ----------- EXP1-2
   *   EXP1-10 ---------- EXP1-1
   *
   *  NOTE: The MISO pin should not get a 5V signal.
   *        To fix, insert a 1N4148 diode in the MISO line.
   */

  #define BEEPER_PIN                 EXP1_10_PIN

  #define SD_DETECT_PIN              EXP2_04_PIN

  #define CLCD_MOD_RESET             EXP2_08_PIN
  #define CLCD_SPI_CS                EXP2_06_PIN
#endif // TOUCH_UI_FTDI_EVE && LCD_FYSETC_TFT81050
